/ ****
MODEL: ZH-A1
1. Maximum Points: 49152 (color area halved)
    Monochrome: 16 * 307 232 * 1536
          48 * 1024
    Color: 16 * 153 632 * 768
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Supports serial communication mode
8. Supports serial program upgrade
9. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-A4
1. Maximum Points: 65536 (color area halved)
    Monochrome: 16 * 409 632 * 2048
          48 * 136 064 * 1024
    Color: 16 * 204 832 * 1024
          48 * 68 064 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Supports serial communication mode
8. Supports serial program upgrade
9. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-Un
1. Maximum Points: 10240 (color area halved)
    Monochrome: 16 * 64 032 * 320
    Color: 16 * 32 032 * 160
2. Support for all scanning
3. Support 4 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-Um
1. Maximum Points: 16384 (color area halved)
    Monochrome: 16 * 102 432 * 512
    Color: 16 * 51 232 * 256
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-Uc
1. Maximum Points: 24576 (color area halved)
    Monochrome: 16 * 153 632 * 768
          48 * 512
    Color: 16 * 76 832 * 384
          48 * 256
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-U0
1. Maximum Points: 32768 (color area halved)
    Monochrome: 16 * 204 832 * 1024
    Color: 16 * 102 432 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-U1
1. Maximum Points: 49152 (color area halved)
    Monochrome: 16 * 307 232 * 1536
48 * 1024
    Color: 16 * 153 632 * 768
          48 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-UF
1. Maximum Points: 32768 (color area halved)
    Monochrome: 16 * 204 832 * 1024
          48 * 68 064 * 512
    Color: 16 * 102 432 * 512
          48 * 33 664 * 256
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-U2
1. Maximum Points: 65536 (color area halved)
    Monochrome: 16 * 409 632 * 2048
          48 * 136 064 * 1024
    Color: 16 * 204 832 * 1024
          48 * 68 064 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-U3
1. Maximum Points: 65536 (color area halved)
    Monochrome: 16 * 409 632 * 2048
          48 * 136 064 * 1024
          80 * 81 696 * 680
          128 * 512
    Color: 16 * 204 832 * 1024
          48 * 68 064 * 512
          80 * 40 896 * 336
          128 * 256
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
         PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-U4
1. Maximum Points: 102400 (color area halved)
    Monochrome: 16 * 409 632 * 3200
          48 * 212 864 * 1600
          80 * 128 096 * 1064
          128 * 800
    Color: 16 * 320 032 * 1600
          48 * 106 464 * 800
          80 * 64 096 * 528
          128 * 400
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-U5
1. Maximum Points: 163,840 (color height halved)
    Monochrome: 16 * 409 632 * 409 648 * 300 864 * 2560
          80 * 204 896 * 1704128 * 1280144 * 1136
          160 * 1024 176 * 928 192 * 848 208 * 784
          224 * 728 240 * 680 256 * 640
    Color: 16 * 409 632 * 204 848 * 169 664 * 1280
          80 * 102 496 * 848 128 * 640
  Note: 12 interface with 8 rows high 08 interface with 4 rows high

2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
Model: ZH-U6
1. Maximum Points: 524288 (color area halved)
    Monochrome: 32 409 696 * 409 664 * 128 * 4096 * 4096
          144 * 3640160 * 3272176 * 2976192 * 2728
          208 * 2520224 * 2336240 * 2184256 * 2048
    Color: 32 * 409 664 * 409 696 * 2728128 * 2048
          144 * 1816160 * 1632176 * 1488192 * 1360
          208 * 1256224 * 1168240 * 1088256 * 1024
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
Model: ZH-U7
1. Maximum Points: 524288 (color area halved)
    Monochrome: 32 409 696 * 409 664 * 128 * 4096 * 4096
          160 * 3272192 * 2728224 * 2336256 * 2048
288 * 1816320 * 1632352 * 1488384 * 1360
          416 * 1256448 * 1168480 * 1088512 * 1024
    Color: 32 * 409 664 * 409 696 * 2728128 * 2048
          160 * 1632192 * 1360224 * 1168256 * 1024
          288 * 904 320 * 816 352 * 744 384 * 680
          416 * 624 448 * 584 480 * 544 512 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
Model: ZH-U8
1. Maximum Points: 1048576 (color area halved)
    Monochrome: 32 * 819 264 * 819 296 * 8192128 * 8192
          160 * 6552192 * 5456208 * 5040224 * 4680
          240 * 4368256 * 4096288 * 3640320 * 3272
          352 * 2976384 * 2728416 * 2520448 * 2336
          480 * 2184512 * 2048
    Color: 32 * 819 264 * 819 296 * 5456128 * 4096
          160 * 3272192 * 2728224 * 2336256 * 2048
          288 * 1816320 * 1632352 * 1488384 * 1360
          416 * 1256448 * 1168480 * 1088512 * 1024
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-E1
1. Maximum Points: 49152 (color area halved)
    Monochrome: 16 * 307 232 * 1536
          48 * 1024
    Color: 16 * 153 632 * 768
          48 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support, Ethernet port and three serial communication mode
8. automatically obtain IP, IP settings without
9. Support single direct connection and LAN communications
10. The network interface is fully compatible direct line of communication and cross-line
11. RS-232 serial communication for direct line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-E3
1. Maximum Points: 65536 (color area halved)
    Monochrome: 16 * 409 632 * 2048
          48 * 136 064 * 1024
          80 * 81 696 * 680
          128 * 512
    Color: 16 * 204 832 * 1024
          48 * 68 064 * 512
          80 * 40 896 * 336
          128 * 256
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support, Ethernet port and three serial communication mode
8. automatically obtain IP, IP settings without
9. Support single direct connection and LAN communications
10. The network interface is fully compatible direct line of communication and cross-line
11. RS-232 serial communication for direct line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-E5
1. Maximum Points: 163,840 (color height halved)
    Monochrome: 16 * 409 632 * 409 648 * 300 864 * 2560
          80 * 204 896 * 1704128 * 1280144 * 1136
          160 * 1024 176 * 928 192 * 848 208 * 784
          224 * 728 240 * 680 256 * 640
    Color: 16 * 409 632 * 204 848 * 169 664 * 1280
          80 * 102 496 * 848 128 * 640
  Note: 12 interface with 8 rows high 08 interface with 4 rows high
     
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support, Ethernet port and three serial communication mode
8. automatically obtain IP, IP settings without
9. Support single direct connection and LAN communications
10. The network interface is fully compatible direct line of communication and cross-line
11. RS-232 serial communication for direct line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-E6

1. Maximum Points: 524288 (color area halved)
    Monochrome: 32 409 696 * 409 664 * 128 * 4096 * 4096
          144 * 3640160 * 3272176 * 2976192 * 2728
          208 * 2520224 * 2336240 * 2184256 * 2048
    Color: 32 * 409 664 * 409 696 * 2728128 * 2048
          144 * 1816160 * 1632176 * 1488192 * 1360
          208 * 1256224 * 1168240 * 1088256 * 1024
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support, Ethernet port and three serial communication mode
8. automatically obtain IP, IP settings without
9. Support single direct connection and LAN communications
10. The network interface is fully compatible direct line of communication and cross-line
11. RS-232 serial communication for direct line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-E7

1. Maximum Points: 524288 (color area halved)
    Monochrome: 32 409 696 * 409 664 * 128 * 4096 * 4096
          160 * 3272192 * 2728224 * 2336256 * 2048
288 * 1816320 * 1632352 * 1488384 * 1360
          416 * 1256448 * 1168480 * 1088512 * 1024
    Color: 32 * 409 664 * 409 696 * 2728128 * 2048
          160 * 1632192 * 1360224 * 1168256 * 1024
          288 * 904 320 * 816 352 * 744 384 * 680
          416 * 624 448 * 584 480 * 544 512 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support, Ethernet port and three serial communication mode
8. automatically obtain IP, IP settings without
9. Support single direct connection and LAN communications
10. The network interface is fully compatible direct line of communication and cross-line
11. RS-232 serial communication for direct line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-E8
1. Maximum Points: 1048576 (color area halved)
    Monochrome: 32 * 819 264 * 819 296 * 8192128 * 8192
          160 * 6552192 * 5456208 * 5040224 * 4680
          240 * 4368256 * 4096288 * 3640320 * 3272
          352 * 2976384 * 2728416 * 2520448 * 2336
          480 * 2184512 * 2048
    Color: 32 * 819 264 * 819 296 * 5456128 * 4096
          160 * 3272192 * 2728224 * 2336256 * 2048
          288 * 1816320 * 1632352 * 1488384 * 1360
          416 * 1256448 * 1168480 * 1088512 * 1024
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support, Ethernet port and three serial communication mode
8. automatically obtain IP, IP settings without
9. Support single direct connection and LAN communications
10. The network interface is fully compatible direct line of communication and cross-line
11. RS-232 serial communication for direct line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-Gm
1. Maximum Points: 16384 (color area halved)
    Monochrome: 16 * 1024
    Color: 16 * 512
2. Support 1 / 4,1 / 8,1 / 16 scan
3. Support free partition
4. Support magical run edge (full screen / partition)
5. Support the countdown, temperature
6. Communication Interface: GPRS RS-232 U disk
7. U disk storage format supports all FAT32 / NTFS / EXFAT
8. U disk support program upgrade
9. Timer switch support
10. Full screen test support
11. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-G0
1. Maximum Points: 32768 (color area halved)
    Monochrome: 16 * 204 832 * 1024
    Color: 16 * 102 432 * 512
2. Support 1 / 4,1 / 8,1 / 16 scan
3. Support free partition
4. Support magical run edge (full screen / partition)
5. Support the countdown, temperature
6. Communication Interface: GPRS RS-232 U disk
7. U disk storage format supports all FAT32 / NTFS / EXFAT
8. U disk support program upgrade
9. Timer switch support
10. Full screen test support
11. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-G2
1. Maximum Points: 65536 (color area halved)
    Monochrome: 16 * 409 632 * 2048
          48 * 136 064 * 1024
    Color: 16 * 204 832 * 1024
          48 * 68 064 * 512
2. Support 1 / 4,1 / 8,1 / 16 scan
3. Support free partition
4. Support magical run edge (full screen / partition)
5. Support the countdown, temperature
6. Communication Interface: GPRS RS-232 U disk
7. U disk storage format supports all FAT32 / NTFS / EXFAT
8. U disk support program upgrade
9. Timer switch support
10. Full screen test support
11. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-G3
1. Maximum Points: 65536 (color area halved)
    Monochrome: 16 * 409 632 * 2048
          48 * 136 064 * 1024
          80 * 81 696 * 680
          128 * 512
    Color: 16 * 204 832 * 1024
          48 * 68 064 * 512
          80 * 40 896 * 336
          128 * 256
2. Support 1 / 4,1 / 8,1 / 16 scan
3. Support free partition
4. Support magical run edge (full screen / partition)
5. Support the countdown, temperature
6. Communication Interface: GPRS RS-232 U disk
7. U disk storage format supports all FAT32 / NTFS / EXFAT
8. U disk support program upgrade
9. Timer switch support
10. Full screen test support
11. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-G4
1. Maximum Points: 144,384 (color area halved)
    Monochrome: 16 * 409 632 * 409 648 * 300 864 * 2560
          80 * 204 896 * 1704128 * 1280
    Color: 16 * 409 632 * 204 848 * 169 664 * 1280
          80 * 102 496 * 848 128 * 640
2. Support 1 / 4,1 / 8,1 / 16 scan
3. Support free partition
4. Support magical run edge (full screen / partition)
5. Support the countdown, temperature
6. Communication Interface: GPRS RS-232 U disk
7. U disk storage format supports all FAT32 / NTFS / EXFAT
8. U disk support program upgrade
9. Timer switch support
10. Full screen test support
11. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5

/ ****
Model: ZH-G7
1. Maximum Points: 524288 (color area halved)
    Monochrome: 32 409 696 * 409 664 * 128 * 4096 * 4096
          160 * 3272192 * 2728224 * 2336256 * 2048
288 * 1816320 * 1632352 * 1488384 * 1360
          416 * 1256448 * 1168480 * 1088512 * 1024
    Color: 32 * 409 664 * 409 696 * 2728128 * 2048
          160 * 1632192 * 1360224 * 1168256 * 1024
          288 * 904 320 * 816 352 * 744 384 * 680
          416 * 624 448 * 584 480 * 544 512 * 512
2. Support 1 / 4,1 / 8,1 / 16 scan
3. Support free partition
4. Support magical run edge (full screen / partition)
5. Support the countdown, temperature
6. Communication Interface: GPRS RS-232 U disk
7. U disk storage format supports all FAT32 / NTFS / EXFAT
8. U disk support program upgrade
9. Timer switch support
10. Full screen test support


/ ****
MODEL: ZH-Wn
1. Maximum Points: 10240 (color area halved)
    Monochrome: 16 * 64 032 * 320
    Color: 16 * 32 032 * 160
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-Wm
1. Maximum Points: 16384 (color area halved)
    Monochrome: 16 * 102 432 * 512
    Color: 16 * 51 232 * 256
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-W0
1. Maximum Points: 32768 (color area halved)
    Monochrome: 16 * 204 832 * 1024
    Color: 16 * 102 432 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-W1
1. Maximum Points: 49152 (color area halved)
    Monochrome: 16 * 307 232 * 1536
          48 * 1024
    Color: 16 * 153 632 * 768
          48 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-W2
1. Maximum Points: 65536 (color area halved)
    Monochrome: 16 * 409 632 * 2048
          48 * 136 064 * 1024
    Color: 16 * 204 832 * 1024
          48 * 68 064 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-W3
1. Maximum Points: 65536 (color area halved)
    Monochrome: 16 * 409 632 * 2048
          48 * 136 064 * 1024
          80 * 81 696 * 680
          128 * 512
    Color: 16 * 204 832 * 1024
          48 * 68 064 * 512
          80 * 40 896 * 336
          128 * 256
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-W4
1. Maximum Points: 102400 (color area halved)
    Monochrome: 16 * 409 632 * 3200
          48 * 212 864 * 1600
          80 * 128 096 * 1064
          128 * 800
    Color: 16 * 320 032 * 1600
          48 * 106 464 * 800
          80 * 64 096 * 528
          128 * 400
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-W5
1. Maximum Points: 163,840 (color height halved)
    Monochrome: 16 * 409 632 * 409 648 * 300 864 * 2560
          80 * 204 896 * 1704128 * 1280144 * 1136
          160 * 1024 176 * 928 192 * 848 208 * 784
          224 * 728 240 * 680 256 * 640
    Color: 16 * 409 632 * 204 848 * 169 664 * 1280
          80 * 102 496 * 848 128 * 640
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-W6

1. Maximum Points: 524288 (color area halved)
    Monochrome: 32 409 696 * 409 664 * 128 * 4096 * 4096
          144 * 3640160 * 3272176 * 2976192 * 2728
          208 * 2520224 * 2336240 * 2184256 * 2048
    Color: 32 * 409 664 * 409 696 * 2728128 * 2048
          144 * 1816160 * 1632176 * 1488192 * 1360
          208 * 1256224 * 1168240 * 1088256 * 1024
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
Model: ZH-W7
1. Maximum Points: 524288 (color area halved)
    Monochrome: 32 409 696 * 409 664 * 128 * 4096 * 4096
          160 * 3272192 * 2728224 * 2336256 * 2048
288 * 1816320 * 1632352 * 1488384 * 1360
          416 * 1256448 * 1168480 * 1088512 * 1024
    Color: 32 * 409 664 * 409 696 * 2728128 * 2048
          160 * 1632192 * 1360224 * 1168256 * 1024
          288 * 904 320 * 816 352 * 744 384 * 680
          416 * 624 448 * 584 480 * 544 512 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT